1178644061	68.0.120.35	C	geda:faq-pcb	davidcary	created	
1180060046	127.0.0.1	E	geda:faq-pcb		external edit	
1180106577	68.0.120.35	E	geda:faq-pcb	davidcary	+footprints	
1185365376	130.75.103.207	E	geda:faq-pcb	kaimartin		
1185366102	130.75.103.207	E	geda:faq-pcb	kaimartin	raise the layer of formating to get an edit button per question. Remove spurious space in front of question mark 	
1185366706	130.75.103.207	E	geda:faq-pcb	kaimartin	Add rename-FAQ	
1235835409	68.0.124.33	E	geda:faq-pcb	davidcary		
1294195740	89.182.210.219	E	geda:faq-pcb	kaimartin	[Is it true that pcb has no concept of a solder mask or paste mask layer?] 	
1317119933	195.34.238.138	e	geda:faq-pcb	vzh	More nice links	
1329768895	127.0.0.1	E	geda:faq-pcb		external edit	
1331245928	178.234.68.179	E	geda:faq-pcb	vzh	Add link to the PCB manual	
1357847065	173.62.216.220	e	geda:faq-pcb	ptay	[How do I install pcb?]  cleaned up text	
1357847130	173.62.216.220	E	geda:faq-pcb	ptay	[Is it true that pcb is limited to exactly 8 copper layers and 2 silkscreen layers?] 	
1357847203	173.62.216.220	E	geda:faq-pcb	ptay	[Is there any relation between the gEDA PCB and the opencircuitdesign PCB?] 	
1357847656	173.62.216.220	E	geda:faq-pcb	ptay	added link to DJ's documentation of PCB	
1397836413	95.179.12.229	e	geda:faq-pcb	vzh	Add link to Russian translation	
1398437395	95.179.41.244	e	geda:faq-pcb	vzh	Add FIXME	
